Application Python/VB/VC On PC/Raspberry Pi

Encoder/Extensometer/Proxy

Temperature Sensor

Torque Sensor (4 Pin)

Load Cell (4 Pins)

This is Serial / Modbus Communication from Controller to PC

RS232

/485/USB

Controllers (Program Inside, IO ports)